{"text_format":"3","workbook":"xlsx","n_sheets":5,"sheets":["Tiltel","Electrical Work","Civil Work LV","Civil Work MV","Civil Work IT System"],"not_rendered":{"images":3,"external_links":16,"defined_names":154},"read":"whole","date_system":"1900"}

{"sheet":"Tiltel","index":0,"n_rows":5,"n_cols":1,"rows_kept":5,"merged":[[0,0,0,2],[1,0,1,2],[2,0,2,2],[3,0,3,2],[4,0,4,2],[5,0,5,2],[6,0,6,2]]}
["CIVIL ENGINEER VERSE"]
["BOQ "]
["Civil Work / Utillity Works / Plumbing Work / Electric Work"]
["Business City"]
["BILL OF QUANTITIES"]

{"sheet":"Electrical Work","index":1,"n_rows":43,"n_cols":6,"rows_kept":43,"merged":[[29,1,29,4],[32,1,32,5],[42,1,42,4]]}
[]
["Item No.","Description","Unit","Qty","Rate (Rs.)","Amount (Rs.)"]
["Bill\nNo. 16","Electrical Works (Road/Street Lighting Network based on LED Road Lighting Fixtures MV, LV etc)"]
[null,"Design,   supply,   transportation,  storage,  installation,   testing   and commissioning of the following items of work, including all material, labour, tools and accessories etc. required for proper completion of each item as  per specification,  drawings and/or  as directed  by the Engineer."]
["801(a)","10m high single arm octagonal shape electric street light pole, made of hot dipped 4.5 mm thick (7 SWG) galvanized steel, tappered from 225  mm  at  bottom  to  100  mm  at  top,with 1500  mmx60  mmx4mm thick   dia.   arm   for   luminaire   installation,   duly   G.I.welded   with 470x470x20 mm base plate with the help of 4 no triangular stiffeners 100x350x20 mm of GI sheet,with built in junction box with shutter & one (01) no. 2A SP MCB 10kA breaker, i/c the cost of nuts & J-rag bolts,  duly  fixed  in  prelaid  concrete  foundation,  foundation  will  be paid additionally as approved and directed by the Engineer Incharge.","Each",{"v":1,"d":"1.00"}]
["801(b)","10m  high  double  arm  octagonal  shape  electric  street  light  pole, made  of  hot  dipped  4.5  mm  thick  (7  SWG)  galvanized  steel, tappered from 225 mm at bottom to 100 mm at top,with 1500 mmx60 mm x4mm  thick dia. arm for luminaire  installation, duly G.I.welded with  470x470x20  mm  base  plate  with  the  help  of  4  no  triangular stiffeners 100x350x20 mm of GI sheet,with built in junction box with shutter  &  two  (02)  nos. 2A  SP MCB  10kA  breaker,  i/c the  cost of nuts   &   J-rag   bolts,   duly   fixed   in   prelaid   concrete   foundation, foundation will be paid additionally as approved and directed by the Engineer Incharge.","Each",{"v":40,"d":"40.00"},{"v":141543,"d":"141,543"}]
["801(c)","12m high single arm octagonal shape electric street light pole, made of hot dipped 4.5 mm thick (7 SWG) galvanized steel, tappered from 225  mm  at  bottom  to  100  mm  at  top,with 1500  mmx60  mmx4mm thick   dia.   arm   for   luminaire   installation,   duly   G.I.welded   with 470x470x20 mm base plate with the help of 4 no triangular stiffeners 100x350x20 mm of GI sheet,with built in junction box with shutter & one (01) no. 2A SP MCB 10kA breaker, i/c the cost of nuts & J-rag bolts,  duly  fixed  in  prelaid  concrete  foundation,  foundation  will  be paid additionally as approved and directed by the Engineer Incharge.","Each",{"v":100,"d":"100.00"},1]
["801(d)","12m  high  double  arm  octagonal  shape  electric  street  light  pole, made  of  hot  dipped  4.5  mm  thick  (7  SWG)  galvanized  steel, tappered from 225 mm at bottom to 100 mm at top,with 1500 mmx60 mm x4mm  thick dia. arm for luminaire  installation, duly G.I.welded with  470x470x20  mm  base  plate  with  the  help  of  4  no  triangular stiffeners 100x350x20 mm of GI sheet,with built in junction box with shutter  &  two  (02)  nos. 2A  SP MCB  10kA  breaker,  i/c the  cost of nuts   &   J-rag   bolts,   duly   fixed   in   prelaid   concrete   foundation, foundation will be paid additionally as approved and directed by the Engineer Incharge.","Each",{"v":164,"d":"164.00"}]
["801(e)","15  m  high  conical  octagonal  (hot  dip)  galvanized  steel  pole  with circular angular top 4 Nos. luminaire arrangement, base plate, J-rag bolts, 2 Amp 04 Nos. SP MCB, pole numbering and earthing etc. as shown on drawing.","Each",{"v":2,"d":"2.00"}]
["801(f)","Road Lighting Pole Foundation","Each",{"v":307,"d":"307.00"}]
[null,"Road Lights & Accessories for Flood Light Installation"]
["802(a)","Road Lighting LED Cobra-head Luminaries of 90W and  120 lm/W conforming  to  IP  66  &  IK  08  or  above  Philips/Osram/Thorn  or NEECA approved  equivalent  manufacturer  with  corrosion  resistant die casted Aluminum housing, silicon  gasket in special groove, UV stable  &  scratch  resistant  synthetic  materials,  thermally  hardened glass  complete  with  LED  Chip  (Philips  Lumiled/Cree/Nichia/Osram make  or  equivalent  approved  manufacturer),  programmable  LED driver  (Harvard/TCI/Lumotech/Philips/VOSSLOH  Schwabe/Lightech make  or  approved equivalent manufacturer), minimum  10kV  surge protection rating i/c the cost of all accessories/ components required for  proper  operation,  fully  flexible  for  future  upgradation  and  easy replacements  for  maintenance  purposes,  bucket  elevator  charges as approved and directed by the Engineer Incharge.","No.",{"v":82,"d":"82.00"}]
["802(b)","Road Lighting LED Cobra-head Luminaries of 120W and  120 lm/W conforming  to  IP  66  &  IK  08  or  above  Philips/Osram/Thorn  or NEECA approved  equivalent  manufacturer  with  corrosion  resistant die casted Aluminum housing, silicon  gasket in special groove, UV stable  &  scratch  resistant  synthetic  materials,  thermally  hardened glass  complete  with  LED  Chip  (Philips  Lumiled/Cree/Nichia/Osram make  or  equivalent  approved  manufacturer),  programmable  LED driver  (Harvard/TCI/Lumotech/Philips/VOSSLOH  Schwabe/Lightech make  or  approved equivalent manufacturer), minimum  10kV  surge protection rating i/c the cost of all accessories/ components required for  proper  operation,  fully  flexible  for  future  upgradation  and  easy replacements  for  maintenance  purposes,  bucket  elevator  charges as approved and directed by the Engineer Incharge.","No.",{"v":296,"d":"296.00"},{"v":72616.9,"d":"72,616.90"}]
["802(c)","Road Lighting LED Cobra-head Luminaries of 150W and  120 lm/W conforming  to  IP  66  &  IK  08  or  above  Philips/Osram/Thorn  or NEECA approved  equivalent  manufacturer  with  corrosion  resistant die casted Aluminum housing, silicon  gasket in special groove, UV stable  &  scratch  resistant  synthetic  materials,  thermally  hardened glass  complete  with  LED  Chip  (Philips  Lumiled/Cree/Nichia/Osram make  or  equivalent  approved  manufacturer),  programmable  LED driver  (Harvard/TCI/Lumotech/Philips/VOSSLOH  Schwabe/Lightech make  or  approved equivalent manufacturer), minimum  10kV  surge protection rating i/c the cost of all accessories/ components required for  proper  operation,  fully  flexible  for  future  upgradation  and  easy replacements  for  maintenance  purposes,  bucket  elevator  charges as approved and directed by the Engineer Incharge.","No.",{"v":132,"d":"132.00"}]
["802(d)","Road Lighting LED Cobra-head Luminaries of 180W and  120 lm/W conforming  to  IP  66  &  IK  08  or  above  Philips/Osram/Thorn  or NEECA approved  equivalent  manufacturer  with  corrosion  resistant die casted Aluminum housing, silicon  gasket in special groove, UV stable  &  scratch  resistant  synthetic  materials,  thermally  hardened glass  complete  with  LED  Chip  (Philips  Lumiled/Cree/Nichia/Osram make  or  equivalent  approved  manufacturer),  programmable  LED driver  (Harvard/TCI/Lumotech/Philips/VOSSLOH  Schwabe/Lightech make  or  approved equivalent manufacturer), minimum  10kV  surge protection rating i/c the cost of all accessories/ components required for  proper  operation,  fully  flexible  for  future  upgradation  and  easy replacements  for  maintenance  purposes,  bucket  elevator  charges as approved and directed by the Engineer Incharge.","No.",{"v":2,"d":"2.00"}]
["802(e)","Flood   Lighting   LED   Luminaries   120W   make   Signify   (Philips), Schreder,  Tungsram  (GE)  or  equivalent  suitable  for  M-2  &  M-3 roads  of  wattage  suitable  for  the  project  requirements,  fully  IP  65 with corrosion resistant die  cast aluminum  housing, silicon gas kit, thermally   hardened   glass   complete   with   LED   drivers,   surge protection and all accessories/ components  required for the proper operation  of  the  system.  The  luminaries  shall  be  fully  flexible  for future upgrades and easy replacements for maintenance purposes. Contractor  to  submit  lighting  design  calculation  as  per  the  offered light fixtures.","No.",{"v":5,"d":"5.00"},{"v":70753,"d":"70,753.00"}]
[null,"Conduits / Pipes"]
["803(a)","PVC pipe/conduit Class-D 100 mm dia with accessories suitable for laying   multi-core   cables   in   trenches/directly   burried   on   road crossings including excavation.","Rm",{"v":2500,"d":"2,500.00"},2]
["803(b)\n803(c)","PVC pipe/conduit Class-B 100 mm dia  with accessories suitable for laying multi-core cables in walls/barriers/structure.\nPVC pipe/conduit Class-B 100 mm dia  with accessories suitable for laying  multi-core   cables   from  pole   to  pole   in  trenches/directly burried including excavation.","Rm\nRm","125.00\n10,250.00"]
[null,"Low Voltage Power Cables"]
["804 (a)","Single core 70mm2 PVC insulated copper  conductor 450/750 volts cable,   in   prelaid   PVC   pipe/M.S.   conduit/G.I   pipe/wooden   strip batten/wooden casing an capping/G.I. wire/trenches (rate for cables only)","Rm",{"v":25,"d":"25.00"}]
["804 (b)","PVC insulated,  PVC  sheathed  4 core  70  mm2,  600/1000  volt  non armoured copper conductor cable for service connection, in prelaid pipe/G.I. wire/trenches, etc. (rate for cable only)","Rm",{"v":1750,"d":"1,750.00"}]
["804 (c)","Single core 35mm2 PVC insulated copper  conductor 450/750 volts cable,   in   prelaid   PVC   pipe/M.S.   conduit/G.I   pipe/wooden   strip batten/wooden casing an capping/G.I. wire/trenches (rate for cables only)","Rm",{"v":1825,"d":"1,825.00"}]
["804(d)","PVC insulated,  PVC  sheathed  4 core  16  mm2,  600/1000  volt  non armoured copper conductor cable for service connection, in prelaid pipe/G.I. wire/trenches, etc. (rate for cable only)","Rm",{"v":11625,"d":"11,625.00"}]
["804 (e)","Single core 16mm2 PVC insulated copper  conductor 450/750 volts cable,   in   prelaid   PVC   pipe/M.S.   conduit/G.I   pipe/wooden   strip batten/wooden casing an capping/G.I. wire/trenches (rate for cables only)","Rm",{"v":11625,"d":"11,625.00"}]
["804(f)","3  Nos.  1  core  2.5  mm2   Cu/PVC  450/750  Voltage  grade  cable (stranded   conductor)   (Imported   copper   shall   be   used.   Verified documentary   evidence   for   source   of   copper   &   PVC   shall   be furnished  prior  to  manufacturing)  from  junction  box  to  the  fitting through the hollow of pole."]
["i","For 10m Pole","No.",{"v":40,"d":"40.00"}]
["ii\niii","For 12m Pole\nFor 15m Pole","No.\nNo.","264.00\n2.00",1]
[805,"Road lighting control panel with angle iron frame cladded 14 SWG, sheet steel enclosure having high quality powder coated paint, color RAL 7032. The  LCP  shall be  complete with incoming and outgoing MCCBs,  Cu bus bars,   magnetic   contactors,   photo-electric   switches,   meters,   indication lights, construction with IP 54 protection class, door, locking arrangement etc. and all other accessories as required for quality work.\nMATERIAL\n1 No. incoming 100 Amp.(adj.) TP, MCCB, 25 kA 6 No. outgoing 25 Amp. (adj.) TP MCCBs, 25 kA\n2 No. outgoing 25 Amp. (adj.) TP MCCBs, 25 kA (Spare) 6 No. 32 Amp. magnetic contactor AC-3\n2 No. 32 Amp. magnetic contactor AC-3 (Spare)\n3 No. photo-electric switches with timers and relays\na) 1 No. ammeters  0-100  Amp, with selector switch (04 position) and CT of 100/5 Amp\nb) 3 No. indication lights\nc) 1 No. voltmeter with fuse and 7 position selector switch.\nd) 3 Ph, N & Earth copper bus bars Internal wiring & line-up terminals etc.\nBrass cable glands/accessories\ne)  08  Nos.  Auto-Manual-OFF  (3  position  switches  for  operation  in  auto (with photocell) and normal (manual mode-photocell  override)\nf) 08 Nos.ON & 08 Nos. OFF push button switch's with indication lights\ng) Panel Light with limit Switch","Job",{"v":4,"d":"4.00"},"501,749 00"]
[null,"Total of MRS"]
[null,"N-MRS ITEMS"]
[806,"Earth point comprising of 10 ft. 5/8\" dia. (16 mm dia) copper coated\nM.S.  rods  driven  in  ground  near  each  lighting  control  panel.  The earthing rods shall be completed with fixing clamps etc.","Each",{"v":8,"d":"8.00"}]
[null,"Transformer, Allied MV Network & Bore Type Earthing (Item no. 807, 808, 809)\nNote: The referred Road Lighting Network shall be fed from the nearby power supply source. In case, nearby power supply source is not available, a dedicated 100 kVA pad mounted distribution transformer and allied MV network shall be installed and payment to the Contractor shall be made accordingly."]
[807,"Transformer"]
["As per WAPDA\nSpecs.","Supply of 100 kVA, 11/0.415 kV pad mounted transformer (with HT & LT Compartment) with foundation and all accessories, Installation and   Connection   Charges   with   energy   meter   as   per   WAPDA\nstandards and practice.","Job",{"v":1,"d":"1.00"},{"v":3509376,"d":"3,509,376"}]
[808,"MV Cable and Termination Kit"]
["a)","MV    cable    3-core    120mm²    XLPE/PVC/SWA/PVC    cable    with aluminium conductor voltage grade:8.7/15 kV","Rm",{"v":200,"d":"200.00"},{"v":13,"d":"13."}]
["b)","Providing and fixing/installation indoor 3-core 120mm², 11KV, XLPE, heat shrink termination Kit complete in all respect as required.","Job",{"v":1,"d":"1.00"},{"v":39372,"d":"39,372.00"}]
["c)","Providing   and   fixing/installation   outdoor   3-core   120mm²   ,11KV, XLPE,   heat   shrink   termination   Kit   complete   in   all   respect   as required.","Job",{"v":1,"d":"1.00"},{"v":43614,"d":"43,614.00"}]
[809,"Bore Type Earthing for Pad Mounted Transformer"]
["a)\n-\n-\n-\n-\n-\n-","Bore  type,  earthing   up  to  permanent  water  level/moist  soil  by arrangement   of  earth  pit/point  comprising  of   concrete/brickwork housing with lifting cover 50mm perforated GI pipe, appropriate bare copper stranded conductor as per details  in drawing.  The earthing and  bonding  shall  be  complete  with  fixing  clamps  etc.  &  all  metal works shall be bonded to the proposed earthing network.\nMATERIAL\nDrilling  of  earth  bore  3\"  dia  100  ft.  deep  or  up  to  permanent  water table.\nSupply and installation of G.I pipe 2\" dia 14 SWG to be installed in pre- made bore including all accessories like tees, bends, sockets etc. Pipe shall  be  connected  to  tinned  copper  spike  as  per  detail  shown  on drawing, complete in all respects.\nSupply and installation  of tinned copper  spike  to be  manufactured as per  detail  shown  on  drawing.  Spike  shall  be  connected/screwed  at bottom   of   G.I   pipe   including   all   accessories   like  nuts   and   bolts complete in all respect.\nSupply  and  installation  of  2  Nos.  70  mm2  bare  stranded  electrolytic copper  conductor  lead  in  prelaid  G.I  pipe  and  connected  to  tinned copper  spike  as  shown   on   drawing.  02Nos.leads  to   be  installed including all accessories like brass nuts, bolts, washers etc complete in all respect.\nSupply and installation of tinned earth test link in earthing pit consisting of  copper  plate  (12\"x2\"x1/2\")  with  fixing  arrangement  on  the  wall  of man hole including brass nuts, bolts washers lugs etc. complete in all respect.\nConstruction  of  earthing  pit  (manhole)  of  internal  size  18\"x18\"x24\" deep  with  9\" thick brick wall  with  cement  mortar,  internal  plaster  1:4, RCC 4\" thick cover with lifting hooks including all accessories complete\nin all respect.","Job",{"v":2,"d":"2.00"}]
["-","Testing and commissioning of the earthing system alongwith all testing accessories complete in all respect."]
[null,"Total of N-MRS"]

{"sheet":"Civil Work LV","index":2,"n_rows":21,"n_cols":6,"rows_kept":21,"merged":[[20,0,20,4]]}
[]
["Sr.\nNo.","Item Description","Unit","Quantity","Rate (Rs.)","Amount (Rs.)"]
[null,"Civil Work Low Voltage"]
[1,"Excavation of trenches in all kinds of soil, except cutting rock, for watersupply pipelines/electric cables upto 5 ft. (1.5 m) depth from ground level, including backfilling, trimming, dressing sides,leveling the beds of trenches to correct grade and cutting pits for joints, etc. complete in all respects.","CM",{"v":26129,"d":"26,129.00"}]
[2,"Supplying and filling sand under floor; or plugging in wells.","CM",{"v":4026.3,"d":"4,026.30"}]
[3,"Rehandling of earthwork:\na) Lead upto a single throw of Kassi, phaorah or shovel","CM",{"v":9395,"d":"9,395.00"}]
[4,"Compaction of earthwork (soft, ordinary or hard soil) :-"]
[null,"a) Mixing, moistening earth to optimum moisture content in layers\nfor compaction, etc. complete.","CM",{"v":9395,"d":"9,395.00"}]
[null,"c) Ramming earthwork (all types of soil).","CM",{"v":18789,"d":"18,789.00"}]
[5,"Cement concrete plain including placing compacting, finishing and curing complete (including screening and washing of stone aggregate):\nf)  Ratio 1:2:4","CM",{"v":5130,"d":"5,130.00"}]
[6,"Placing, compacting, finishing and curing of concrete using Ordinary Portland Cement / Sulphate resisting cement / Slag cement as may be required; including screening, washing of aggregates and mixing of constituents using batching plant, Transportation by transit mixer, pouring with pump in the required proportions to achieve a nominal cylindrical strength in the field as per ACI214, with the specified consistency. i/c the cost of shuttering, compaction with Viberator, excluding the cost of Admixture, as approved and directed by the Engineer Incharge."]
[null,"( c) Substructure (Foundations, Raft, Strip and Footing Beams"]
[null,"vi) 3000 PSI","CM",{"v":9,"d":"9.00"},{"v":25386.51,"d":"25,386.51"}]
[null,"(b) Retaining/ Shear walls laid in situ or precast laid in position, or prestressed members cast ( Formwork on both sides)\nv) 3000 PSI\n(i) Upto 9\" thick","CM",{"v":3,"d":"3.00"},"30,2"]
[7,"(e) Erecting and fixing in position, precast cement concrete or\nstone slab in roofs or lintels, etc. lift upto 20 ft., (6m) including all charges.","CM",{"v":3,"d":"3.00"}]
[8,"Fabrication of mild steel reinforcement for cement concrete including cutting, bending, laying in position, making joints and fastenings including cost of binding wire and labour charges for binding of steel reinforcement (also includes removal of rust from\nbars):-"]
[null,"(c) Deformed bars (Grade-60)","Ton",1.11]
[9,"Bitumen coating to plastered or cement concrete surface:-\ni) 20 lbs. per 100 Sft. (9.07 Kg per Sq.m)","SM",{"v":36942,"d":"36,942.00"}]
[10,"Providing, laying, cutting, jointing and testing pipe line in trenches with PVC/ uPVC pipes of B.S.S. with `D' Class complete in all respects:-"]
[null,"c) 4\" i/d (100 mm)","M",{"v":12923,"d":"12,923.00"}]
["TOTAL COST"]

{"sheet":"Civil Work MV","index":3,"n_rows":21,"n_cols":6,"rows_kept":21,"merged":[[20,0,20,4]]}
[]
["Sr.\nNo.","Item Description","Unit","Quantity","Rate (Rs.)","Amount (Rs.)"]
[null,"Civil Work Medium Voltage"]
[1,"Excavation of trenches in all kinds of soil, except cutting rock, for watersupply pipelines/electric cables upto 5 ft. (1.5 m) depth from ground level, including backfilling, trimming, dressing sides,leveling the beds of trenches to correct grade and cutting pits for joints, etc. complete in all respects.","CM",{"v":26896,"d":"26,896.00"}]
[2,"Supplying and filling sand under floor; or plugging in wells.","CM",{"v":8767,"d":"8,767.00"}]
[3,"Rehandling of earthwork:\na) Lead upto a single throw of Kassi, phaorah or shovel","CM",{"v":8069,"d":"8,069.00"}]
[4,"Compaction of earthwork (soft, ordinary or hard soil) :-"]
[null,"a) Mixing, moistening earth to optimum moisture content in layers\nfor compaction, etc. complete.","CM",{"v":8069,"d":"8,069.00"}]
[null,"c) Ramming earthwork (all types of soil).","CM",{"v":8069,"d":"8,069.00"}]
[5,"Cement concrete plain including placing compacting, finishing and curing complete (including screening and washing of stone aggregate):\nf)  Ratio 1:2:4","CM",{"v":2430,"d":"2,430.00"}]
[6,"Placing, compacting, finishing and curing of concrete using Ordinary Portland Cement / Sulphate resisting cement / Slag cement as may be required; including screening, washing of aggregates and mixing of constituents using batching plant, Transportation by transit mixer, pouring with pump in the required proportions to achieve a nominal cylindrical strength in the field as per ACI214, with the specified consistency. i/c the cost of shuttering, compaction with Viberator, excluding the cost of Admixture, as approved and directed by the Engineer Incharge."]
[null,"( c) Substructure (Foundations, Raft, Strip and Footing Beams"]
[null,"vi) 3000 PSI","CM",{"v":16,"d":"16.00"},{"v":25386.51,"d":"25,386.51"}]
[null,"(b) Retaining/ Shear walls laid in situ or precast laid in position, or prestressed members cast ( Formwork on both sides)\nv) 3000 PSI\n(i) Upto 9\" thick","CM",{"v":13,"d":"13.00"},"30,2"]
[7,"(e) Erecting and fixing in position, precast cement concrete or\nstone slab in roofs or lintels, etc. lift upto 20 ft., (6m) including all charges.","CM",{"v":8,"d":"8.00"}]
[8,"Fabrication of mild steel reinforcement for cement concrete including cutting, bending, laying in position, making joints and fastenings including cost of binding wire and labour charges for binding of steel reinforcement (also includes removal of rust from\nbars):-"]
[null,"(c) Deformed bars (Grade-60)","Ton",2.78]
[9,"Bitumen coating to plastered or cement concrete surface:-\ni) 20 lbs. per 100 Sft. (9.07 Kg per Sq.m)","SM",{"v":33365,"d":"33,365.00"}]
[10,"Providing, laying, cutting, jointing and testing pipe line in trenches with PVC/ uPVC pipes of B.S.S. with `D' Class complete in all respects:-"]
[null,"c) 4\" i/d (100 mm)","M",{"v":65326,"d":"65,326.00"}]
["TOTAL COST"]

{"sheet":"Civil Work IT System","index":4,"n_rows":27,"n_cols":6,"rows_kept":27,"merged":[[15,5,18,5],[26,0,26,4]]}
[]
["Sr.\nNo.","Item Description","Unit","Quantity","Rate\n(Rs.)","Amount\n(Rs.)"]
[null,"Civil Work of IT System"]
[1,"Earth work  excavation in  open cutting for sewers  and manholes shown  and  beams,  dressing  to  correct  section  and  dimension according to templates and levels and removing surface water in all  types of soil except shingle, gravel and rock.\ni) 0 ft. to 7.0 ft. (0 to 2.10 m) depth","CM",{"v":295,"d":"295.00"}]
[2,"Excavation of trenches in all kinds of soil, except cutting rock, for watersupply pipelines upto 5 ft. (1.5 m) depth from ground level, including trimming, dressing sides, leveling the beds of trenches to correct grade and cutting\npits for joints, etc. complete in all respects.","CM",{"v":17654,"d":"17,654.00"}]
[3,"Supplying and filling sand under floor; or plugging in wells.","CM",{"v":7180,"d":"7,180.00"}]
[4,"Rehandling of earthwork:\na) Lead upto a single throw of Kassi, phaorah or shovel","CM",{"v":10769,"d":"10,769.00"}]
[5,"Compaction of earthwork (soft, ordinary or hard soil) :-"]
[null,"a) Mixing, moistening earth to optimum moisture content in layers\nfor compaction, etc. complete.","CM",{"v":10769,"d":"10,769.00"}]
[null,"c) Ramming earthwork (all types of soil).","CM",{"v":12244,"d":"12,244.00"}]
[6,"Cement concrete plain including placing compacting, finishing and curing complete (including screening and washing of stone aggregate):\n(i) Ratio 1: 4: 8","CM",{"v":8,"d":"8.00"},"17,79"]
[7,"Placing, compacting, finishing and curing of concrete using Ordinary Portland Cement / Sulphate resisting cement / Slag cement as may be required; including screening, washing of aggregates and mixing of constituents using batching plant, Transportation by transit mixer, pouring with pump in the required proportions to achieve a nominal cylindrical strength in the field as per ACI214, with the specified consistency. i/c the cost of shuttering, compaction with Viberator, excluding the cost of Admixture, as approved and directed by the Engineer Incharge."]
[null,"( c) Substructure (Foundations, Raft, Strip and Footing Beams"]
[null,"vi) 3000 PSI","CM",{"v":22,"d":"22.00"},"25,38"]
[null,"(b) Retaining/ Shear walls laid in situ or precast laid in position, or prestressed members cast ( Formwork on both sides)"]
[null,"v) 3000 PSI\n(i) Upto 9\" thick","CM",{"v":20,"d":"20.00"},"30,27"]
[null,"(e) Erecting and fixing in position, precast cement concrete or"]
[8,"stone slab in roofs or lintels, etc. lift upto 20 ft., (6m) including all","CM",{"v":8,"d":"8.00"}]
[null,"charges."]
[9,"Fabrication of mild steel reinforcement for cement concrete including cutting, bending, laying in position, making joints and fastenings including cost of binding wire and labour charges for binding of steel reinforcement (also includes removal of rust from\nbars):-"]
[null,"(c) Deformed bars (Grade-60)","Ton",3.99]
[10,"Bitumen coating to plastered or cement concrete surface:\ni) 20 lbs. per 100 Sft. (9.07 Kg per Sq.m)","SM",{"v":232,"d":"232.00"}]
[11,"Providing, laying, cutting, jointing and testing pipe line in trenches with PVC/ uPVC pipes of B.S.S. with `D' Class complete in all\nrespects:-"]
[null,"b) 3\" i/d (75 mm)","M",{"v":40,"d":"40.00"}]
[12,"Small iron work, such as gusset plates, knees, bends, stirrups, straps, rings, etc. including cutting, drilling, riveting, handling, assembling and fixing but excluding erection in position.","Kg",{"v":900,"d":"900.00"}]
[13,"Providing, laying, cutting, jointing, testing and disinfecting High Density Polyethylene Pipe (HDPE-100) working presure pipe, Beta / Dadex / Popular / IIL or approved equivalent manufacturer, including the cost of specials, in trenches, as approved & directed by the engineer incharge, complete in all respects.\nb) PN-8 (SDR-21)\n4) 50 mm","RM",{"v":36200,"d":"36,200.00"}]
["TOTAL COST"]