{"text_format":"3","workbook":"xlsx","n_sheets":3,"sheets":["Tiltel","Water Supply & Distribution","Tube Well"],"not_rendered":{"images":1,"external_links":16,"defined_names":154},"read":"whole","date_system":"1900"}

{"sheet":"Tiltel","index":0,"n_rows":5,"n_cols":1,"rows_kept":5,"merged":[[0,0,0,2],[1,0,1,2],[2,0,2,2],[3,0,3,2],[4,0,4,2],[5,0,5,2],[6,0,6,2]]}
["CIVIL ENGINEER VERSE"]
["BOQ "]
["Water Supply System"]
["Business City"]
["BILL OF QUANTITIES"]

{"sheet":"Water Supply & Distribution","index":1,"n_rows":38,"n_cols":6,"rows_kept":38,"merged":[[37,0,37,4]]}
[]
["Sr. No.","Item Description","Unit","Quantity","Rate","Amount (Rs.)"]
["Bill\nNo. 7","Water Supply & Distribution Network"]
[1,"Excavation of trenches in all kinds of soil, except cutting rock, for watersupply pipelines/electric cables upto 5 ft. (1.5 m) depth from ground level, including backfilling, trimming, dressing sides,leveling the beds of trenches to correct grade and cutting pits for joints, etc. complete in all\nrespects.","CM",{"v":224,"d":"224.00"}]
[2,"Supplying and filing sand under floor or plugging well","CM",{"v":24,"d":"24.00"}]
[3,"Rehandling of earth work"]
[null,"a) Lead upto a single throw of Kassi, phaorah or shovel","CM",{"v":168,"d":"168.00"}]
[4,"Compaction of earthwork (soft, ordinary or hard soil) :-"]
[null,"a) Mixing, moistening earth to optimum moisture content in layers for compaction, etc. complete.","CM",{"v":168,"d":"168.00"}]
[null,"c) Ramming earthwork (all types of soil).","CM",{"v":168,"d":"168.00"},7]
[5,"Cement   concrete   plain   including   placing,   compacting,\nfinishing   and   curing   complete   (including   screening   and washing of stone aggregate)"]
[null,"f)  Ratio 1:2:4","CM",{"v":4,"d":"4.00"},"21,77"]
[null,"i)  Ratio 1:4:8","CM",{"v":2,"d":"2.00"},"17,79"]
[6,"Providing and laying reinforced cement concrete (including prestressed concrete), using Ordinary Portland Cement / Sulphate resisting cement / Slag cement as may be required; coarse sand and screened graded and washed aggregate, in required shape and design, including forms, moulds, shuttering, lifting, compacting, curing, rendering and finishing exposed surface, complete (but excluding the cost of steel reinforcement, its fabrication and placing in position, etc.):-"]
[null,"(a) Reinforced cement concrete in roof slab, beams, columns lintels, girders and other structural members laid in situ or precast laid in position, or prestressed members cast in situ, complete in all respects:-\n(c) Type C (nominal mix  1: 2: 4)","CM",{"v":23,"d":"23.00"},"31,22"]
[null,"(c) Reinforced cement concrete in slab of rafts / strip foundation, base slab of column and retaining walls; etc and footing beams, other structural members other than those mentioned in 6(a)&(b) above not requiring form work (i.e. horizontal shuttering) complete in all respects:-\n(3) Type C (nominal mix 1: 2: 4)","CM",{"v":3,"d":"3.00"}]
[7,"Fabrication of mild steel reinforcement for cement concrete including cutting, bending, laying in position, making joints and fastenings including cost of binding wire and labour charges for binding of steel reinforcement (also includes removal of rust from bars):-\n(c) Deformed bars (Grade-60)","Ton",3.06]
[8,"Pacca brick work other than building upto 10ft. (3 m) height.\ni) cement, sand mortar:- Ratio 1:3","CM",{"v":103,"d":"103.00"}]
[9,"Cement plaster 1:4 upto 20' (6.00 m) height:-\nc)  ¾\"  (20 mm) thick","SM",{"v":360,"d":"360.00"}]
[10,"Small iron work, such as gusset plates, knees, bends, stirrups, straps, rings, etc. including cutting, drilling, riveting, handling, assembling and fixing; but including erection in\nposition.","Kg",{"v":1200,"d":"1,200.00"}]
[11,"Providing, laying, cutting, jointing, testing and disinfecting High Density Polyethylene Pipe (HDPE-100) working presure pipe, Beta / Dadex / Popular / IIL or approved equivalent manufacturer, including the cost of specials, in trenches, as approved & directed by the engineer incharge, complete in all respects."]
[null,"c) PN-8 (SDR-21)"]
[null,"32 mm","PM",{"v":77,"d":"77.00"}]
[null,"125 mm","PM",{"v":60,"d":"60.00"}]
[null,"180 mm","PM",{"v":74,"d":"74.00"}]
[null,"225 mm","PM",{"v":74,"d":"74.00"}]
[null,"250 mm","PM",{"v":94,"d":"94.00"}]
[null,"315 mm","PM",{"v":44,"d":"44.00"}]
[null,"355 mm","PM",{"v":41,"d":"41.00"}]
[12,"Making connection for new watersupply lines with the running main, including excavation of trench and refilling, complete, but excluding cost of pipe and specials, etc.\nDiameter of running main:"]
[null,"i) upto 6\" i/d (150 mm)","P.Con",{"v":5,"d":"5.00"}]
[13,"Providing and fixing heavy duty Globe valve of specified dia meter and material for pressure rating PN-16 made of  Crane (USA), Hatersly (UK), Scon (Pakistan) or approved equivalent manufacturer, i/c the cost of all accessories flanges, nut / bolt and gas kit where required complete in all respect as approved and directed by the Engineer Incharge."]
[null,"(a) Brass Threaded Valves"]
[null,"(vi) 2\" dia","Each",{"v":5,"d":"5.00"},{"v":14991,"d":"14,991"}]
[14,"Providing and fixing 6\" thick R.C.C. manhole cover with tee shaped C.I. frame of 22\" I/d (frame weighing 37.324 Kg. or one maund as per Standard Drawing STD/PD No. 6, of\n1977, complete in all respect.","Each",{"v":4,"d":"4.00"},{"v":24825,"d":"24,825.00"}]
[15,"Providing and fixing, air valve 2½ (65mm) dia of B.S.S. quality and weight (complete with jointing material).\nb) double","Each",{"v":2,"d":"2.00"},{"v":14395.8,"d":"14,395.80"}]
[16,"Supply, installation, testing, and commissioning of Garden / fire Hydrants made by Haseen Habib / Teepu Engineering or approved equvilent manufacturer, according to B.S.S.\n750 standard double delivery type having 4\" dia barrel with  2 Nos.2-1/2\" valve including the cost of jointing material with all fittings and accessories complete in all respect as approved by the Engineer Incharge.","Each",{"v":2,"d":"2.00"},"68,76"]
["TOTAL COST"]

{"sheet":"Tube Well","index":2,"n_rows":110,"n_cols":6,"rows_kept":110,"merged":[[3,0,4,0],[3,1,3,2],[3,3,4,3],[3,4,4,4],[3,5,4,5],[18,2,21,2],[18,3,21,3],[18,4,21,4],[18,5,21,5],[109,0,109,4]]}
[]
["Sr.\nNo.","Item Description","Unit","Quantity","Rate","Amount (Rs.)"]
["Bill\nNo. 15","TUBE WELL (3 Cusecs)"]
[null,"INSTALLATIN / CONSTRUCTION OF 3 CUSEC CAPACITY TUBE WELL"]
[null,"DRILLING AND BORING SUB-HEAD-1"]
[1,"Regular excavation dressed for water storage pit\n(35' x 40' x 5')","CM",{"v":198,"d":"198.00"}]
[2,"Direct Rotary/Reverse Rotary drilling of bore for tubewells, in all types of soil except shingle, gravel and rock:-"]
[null,"a) from ground level to 250 ft. (75 m) below ground level:-\nii) 20\" to 26\" (500 to 650 mm) i/d","RM",{"v":75,"d":"75.00"}]
[null,"b) exceeding 250 ft. (75 m) depth below ground level:-\nii) 20\" to 26\" (500 to 650 mm) i/d","RM",{"v":15,"d":"15.00"}]
[null,"b) exceeding 250 ft depth below ground level\ni) 15\" to 18\" (375 to 450 mm) i/d","RM",{"v":96,"d":"96.00"}]
[3,"Furnishing sample of water from bore hole","P/Set 2\nBottles",{"v":50,"d":"50.00"},{"v":232,"d":"232."}]
[4,"Transportation of earth all types when the total distance, including the lead covered in the item of work. (drilled earth from bore hole)","CM",{"v":100,"d":"100.00"},{"v":258,"d":"258."}]
[5,"Providing and installing M.S. blind pipe socketed/welded joint, M.S. reducer (where necessary), in tubewell bore hole, including jointing/welding with strainer, etc. complete:- 15\" i/d, ¼\" (381 mm i/d 6 mm) thick","RM",{"v":83,"d":"83.00"},{"v":26634.25,"d":"26,634.25"}]
[6,"Shrouding  with  graded  pea  gravel  3/8\"  to  1/8\"  (10  to  3mm), around tubewell in bore hole.","CM",{"v":11,"d":"11.00"},{"v":7293.55,"d":"7,293.55"}]
[7,"Testing and developing of tubewell of size 6\" (150 mm)\ni/d and above continuously."]
[null,"i) upto 1.5 cs. Discharge","P/hours",{"v":30,"d":"30.00"},{"v":2693.7,"d":"2,693.70"}]
[null,"ii) above 1.5 cs. Discharge","P/hours",{"v":45,"d":"45.00"},{"v":3253.1,"d":"3,253.10"}]
[8,"Providing   strong   substantially   built   box   of   deodar   wood 4'x2½'x9\" (1200x750x225 mm), with compartments, lock and locking  arrangement,  for  preserving  samples  of  strata  from\nbore hole.","Job",{"v":1,"d":"1.00"},{"v":49399.7,"d":"49,399.70"}]
["9\n","Providing  and installing Fiberglass  Reinforced Polypropelene (FRP)  strainer  of  specifid  wall  thickness  having  slot  size  of 0.9mm to 1.10mm in Tube well bore hole i/c the cost of male / female   coupling  with  Nylone  Strip,   studs   complete   in   all respect as approved and directed by the Engineer Incharge.\nv) 8\" inch dia (5 mm thickness)\nSmall iron work, such as gusset plates, knees, bends stirrups, straps, rings, etc. including cutting, drilling, riveting, handling, assembling and fixing; but excluding erection in position","RM\nKg","61.00\n350.00"]
[null,"Providing  and  fixing   M.S.  cap  to  cover  the  pump   house casing  upto  12\"  dia  1/4\"  thick  including  cutting,  jointing  and\nwelding etc comlete in all respect"]
[null,"M.S Bars size 1/2\" i/d & 2 Nos clamps at right angle 1/2\" thick\n6\"  wide  5  ft  long  for  holding  down  bolts  with  nuts  for  RCC 1:2:4 to house casing concrete block."]
[10,"Providing and fixing M.S centralizers"]
[11,"Providing / laying cement concrete block size as per drawing with RCC ratio 1:2:4 to house casing complete.","CM",{"v":3,"d":"3.00"}]
[12,"Geo physical log survey","Job",{"v":1,"d":"1.00"}]
[null,"SUPPLY   AND   INSTALLATION  OF   VERTICAL   TURBINE PUMP WITH 75 HP MOTOR"]
[null,"Sub Head - ll"]
[null,"TUBE WELL (3 Cusecs)"]
[1,"Supplying Installation testing & commissioning of vertical  shaft deep well turbine pump PECO/ KSB / GROUNDFOS or equivalent approved by HUD & PHE Department (ISO 9001/9002 Certified) with a lowering of 180 ft column pipe and multistage bowl assembly capable to discharge of 3-Cft clear water against a head of 240 ft, pump as per specification.\nSupply / installation of vertical shaft squirrel cage induction type electric motor rating of 75 HP/ 4 pole, 380- 400-V 3- Phase, 50H with non return ratchet insulation Class-F   strictly according to WASA standard specification for electric motor IP 55 manufacture by ABB, PECO / Siemens or equivalent including testinting & commissioning complete in all respect","P.S",{"v":1,"d":"1.00"}]
[2,"Providing / fixing base plate size 3'x3’x1.5\" with centre hole 19\" i/d including drilling of foundation bells discharge head bolts water level measurement holes etc duly finished as\nrequired by the Engineer.","Each",{"v":1,"d":"1.00"},{"v":52887,"d":"52,887.00"}]
[null,"POWER WIRING"]
[null,"SUB-HEAD -III"]
[1,"Supply and erection of single core PVC insulated, PVC sheathed  copper  conductor,  600/1000  volts  grade  cable,  in prelaid  G.I.  pipe  /  M.S.  conduits  /  PVC  pipe  /  G.I.  wire  / trenches, etc (rate for cable only):- (Rate for cable only)"]
[null,"ix) 95 mm sq (37/0.072\")","P/Mtr",{"v":9,"d":"9.00"},{"v":4130.6,"d":"4,130.60"}]
[2,"Supply and erection of 3 pin switch and plug combined, recessed type.\nii) 10/15 amp","Each",{"v":2,"d":"2.00"},214.45]
[3,"Supply  and  erection  of  plain  pendent  lamp  holder,  complete with bakelite lamp holder and flexible twin wire\n23/0.0076\" upto 2 metre length (without bulb and shade).","Each",{"v":4,"d":"4.00"},{"v":426,"d":"426."}]
[4,"Supply  and  erection  of  G.I.  flexible  pipe  for  wiring,  including welding of sockets, nipples and check nuts, etc. complete:-\ni) 80 mm i/d","P/Mtr",{"v":5,"d":"5.00"},{"v":2169.1,"d":"2,169.10"}]
[5,"Supply and erection of PVC pipe for surface wiring (main and sub-main)   including   clamps,  inspection   boxes,  pull  boxes bends etc., complete with all specials:-\ni) 80 mm i/d","P/Mtr",{"v":5,"d":"5.00"}]
[6,"Supply  and  erection  PVC  pipe  for  recessed  wiring  (main andsub-main)   purpose,   including   bends,   specials,   etc.   in floor, wall or trenches:-\ni) 80mm i/d","P/Mtr",{"v":5,"d":"5.00"}]
[7,"Supply and fitting of mercury vapour lamp, complete with choke set.\nii) 250 watt lamp","Each",{"v":8,"d":"8.00"}]
[8,"Supply and erection of tube light, including rod, choke, starter with  frame,  flexible  wire,  including  connection  from  ceiling rose, etc., complete.\nii) single rod (40 watts) with one choke and one starter.","P/Set",{"v":3,"d":"3.00"}]
[9,"Providing and fixing Pakistan Energy Label NEECA approved Copper winded wall bracket Fan i/c the cost of necessary cable and hardware for connection as approved and directed by Engineer Incharge.\nii) 24\" Sweep dia","Each",{"v":1,"d":"1.00"}]
[10,"Providing and fixing Pakistan Energy Label NEECA approved Copper winded Exaust Fan i/c the cost of necessary cable and hardware for connection from ceiling rose complete as approved and directed by Engineer Incharge.\na) Plastic body\n(ii) 12\" dia\nPart B - Earthing (02 No. for each tube well)","Each",{"v":2,"d":"2.00"}]
[null,"TUBE WELL (3 Cusecs)"]
[null,"Providing and  Installation of  special earthing  with distribution copper busbar and 4 SWG wire  copper conductor i/c copper plato 2'x2'x1/4\" thick charcoal, salt and lime (1:2:4), G.l. Pipe, i/c  excavatlon  of  pit  and  other  items  etc.  upto  permanent water  table  having  a  resistance  of  0.5-1.0  ohms  and  each electrical and metalling components will be connected  at two points with earth strip of 3x25mm  fitted throughout inside the wall  at  1  feet  height  connected  with  main  earthing  strip  at main earthing pit by solid copper conductor at minimum three points as per standard specifications. This item also Includes supply  and  erection  of  PVC  pipe  abovo  the  ground  and construction  of  18x18  Inches  chamber  on  base  of  3  Inches RCC 1:4:8 with 4-1/2 Inches thick slab of 1:2:4 complete In all respect for earthing purposos."]
[1,"Direct Rotary/Reverse Rotary drilling of bore for tubewells, in all types of soil except shingle, gravel and rock:-\na) from ground level to 250 ft. (75 m) below ground level:-\nii) 20\" to 26\" (500 to 650 mm) i/d","RM",{"v":12,"d":"12.00"},{"v":4096.8,"d":"4,096.80"}]
[2,"Providing, laying, cutting, jointing, testing and disinfecting G.I. pipeline in trenches, with socket joints, using G.I. pipes of\nB.S.S. 1387-1967 complete in all respects, with specials and valves.\n(Medium Quality)\na) ½\" i/d (15 mm) 2.65mm thick","PM",{"v":6,"d":"6.00"},{"v":770,"d":"770.00"}]
[3,"Supply   and   erection   of   PVC   pipe   for   wiring   on   surface including  clamps  inspection  boxes,  pull  boxes,  bends,  tees, repairing surface, etc., complete with all specials:-\ni) 12 mm i/d.","PM",{"v":6,"d":"6.00"},195.75]
[4,"RCC in roof slab 1:2:4 (2.25x2.25x0.25 = 1.27 Cft)","CM",1,"31,229.83\n303."]
[5,"Fabrication  of  mild  steel  reinforcement  for  cement  concrete including  cutting,  bending,  laying  in  position,  making  joints and  fastenings   including   cost   of  binding  wire  and   labour charges   for   binding  of   steel  reinforcement   (also  includes removal of rust from bars):-","Kg",14]
[null,"(c) Deformed bars (Grade-60)"]
[6,"Pacca brick work in foundation and plinth in:-\ni) Cement, sand mortar:- Ratio 1:4","CM",{"v":1,"d":"1.00"}]
[7,"Rehandling of earth work","CM",{"v":8,"d":"8.00"}]
[null,"PROVIDING AND FIXING OF C.l SPECIALS\nSub Head-IV"]
[1,"Providing and fixing sluice valve of B.S.S. quality and weight, Class  `B',  for  cast  iron  pipe  line,  and  Asbestos  cement  pipe\nline (including cost of jointing material):-"]
[null,"8\" i/d","Each",{"v":8,"d":"8.00"}]
[2,"Providing and fixing cast iron special of B.S.S. Class `B' (such as bend,  tee cross  collar,  reducer,  tail piece,  flanged  spigot, cap, flanged socket, taper, angle branch,\nplug etc.) for cast iron pipe line , complete:-\nb) (C.l flanged and flanged joint)\nii) 8\" to 12\" (200 to 300 mm) i/d","P/Kg",{"v":380,"d":"380.00"}]
[3,"Providing  cement  concrete  /  brick  blocks  to  support  bends with  ratio  1:2:4  i/c  of  screening  washing  of  stone  aggregate shuttering and curing etc complete as per drawing, complete job.\nf)  Ratio 1:2:4","CM",{"v":2,"d":"2.00"}]
[4,"Pacca brick work other than building upto 10ft. (3 m) height. Construction of brick support for tube well delivery pipe as per drawing complete in all respects\ni) cement, sand mortar:- Ratio 1:3","CM",{"v":2,"d":"2.00"}]
[null,"TUBE WELL (3 Cusecs)"]
[5,"Construction  of  RCC  support  for  tube  well delivery  pipe  and bend as per drawing complete in all respects."]
[null,"RCC 1:2:4 on Ground","CM",{"v":1,"d":"1.00"}]
[null,"CONSTRUCTION OF TUBE WELL CHAMBER"]
[null,"Sub Head -V"]
[1,"Excavation   in   foundation   of   building,   bridges   and   other structures,  including  dagbelling,  dressing,  refilling  in  layers around structure with excavated earth, watering and ramming lead upto one chain (30 m) depth upto 5 ft (1.5m).\n2) a) By Excavator\nii) Ordinary soil","CM",{"v":50,"d":"50.00"}]
["2\n","Pacca brick work in foundation and plinth in cement sand mortar.\nRatio 1:4\n","CM\n","33.00\n",{"v":1290.5,"d":"1,290.50"}]
[3,"Providing  and  laying  damp proof  course  of  cement  concrete 1:2:4  (using  cement,  sand  and  shingle),  including  bitumen coating  \n(a) with one coat bitumen and one coat polythene sheet 500 gauge\ni) 1½\" thick (40 mm)","\nSM","\n10.00"]
[4,"Pacca brickwork in ground floor,\ni) cement, sand mortar:- Ratio 1:4","CM",{"v":33,"d":"33.00"},{"v":15271.25,"d":"15,271.25"}]
[5,"Providing and laying reinforced cement concrete (including prestressed concrete), using Ordinary Portland Cement / Sulphate resisting cement / Slag cement as may be required; coarse sand and screened graded and washed aggregate, in required shape and design, including forms, moulds, shuttering, lifting, compacting, curing, rendering and finishing exposed surface, complete (but excluding the cost of steel reinforcement, its fabrication and placing in position, etc.):-"]
[null,"(a) Reinforced cement concrete in roof slab, beams, columns lintels, girders and other structural members laid in situ or precast laid in position, or prestressed members cast in situ, complete in all respects:-\n(c) Type C (nominal mix  1: 2: 4)","CM",{"v":0.5,"d":"0.50"},{"v":31229.83,"d":"31,229.83"}]
[6,"Providing, laying, cutting, jointing, testing and disinfecting PVC/ uPVC pipe line with `B' Class working pressure pipe, in trenches, complete in all respects:-\na) 3\" i/d (75 mm)","RM",{"v":24,"d":"24.00"}]
[7,"Fabrication  of  mild  steel  reinforcement  for  cement  concrete including  cutting,  bending,  laying  in  position,  making  joints and  fastenings   including   cost   of  binding  wire  and   labour charges   for   binding  of   steel  reinforcement   (also  includes removal of rust from bars):-\n(c) Deformed bars (Grade-60)","Kg",{"v":1120,"d":"1,120.00"}]
[8,"Cement plaster 1:4 upto 20' (6.00 m) height:-\nb) ½\" (13 mm) thick","SM",{"v":179,"d":"179.00"}]
[9,"Cement pointing struck joints, on walls, upto 20' (6.00 m) hiehgt:-\nRatio 1:2","SM",{"v":277,"d":"277.00"}]
["10\n","Khassi parnalas in cement, sand mortar 1:2, 12\" (300 mm) outside width finished smooth with a floating coat of\nneat cement.\n","P.M\n","7.00\n"]
[11,"Khuras on roof 2'x2'x6\" (600 x 600 x 150 mm)"]
[12,"Bottom Khuras of brick masonry in cement mortar 1:6, 4'x2'x4½\" (1200x600x113 mm) over 3\" (75 mm) cement\nconcrete 1:4:8.","Each",{"v":2,"d":"2.00"}]
[13,"Dry rammed brick or stone ballast, 1½\" to 2\"( 40 mm to 50\nmm) gauge.","CM",{"v":5,"d":"5.00"}]
[null,"TUBE WELL (3 Cusecs)"]
[14,"Providing and laying conglomerate flooring (two coat work) with top layer of ½\"(13mm) thick wearing surface, consisting of one part of cement and 2 parts of stone chips passing 3/16\"(6 mm) sieve, over bottom layer of\ncement concrete 1:3:6, including surface finishing and dividing in panels:-\n(a) 1½\"(40 mm) thick\n","SM\n","42.00\n"]
["\n15","\nSupply & filling sand under floors or plugging in wells.","\nCM","\n5.00"]
[16,"Single layer  of  tiles  9\"x4½\"x1½\"  (225x113x40  mm)  laid  over 4\"(100   mm)   earth   and   1\"   (25   mm)   mud   plaster   without Bhoosa,  grouted  with  cement  sand  1:3  on  top  of  RCC  roof slab, provided with 34 lbs. per %Sft. or 1.72 Kg/Sq.m bitumen\ncoating sand blinded.","SM",{"v":43,"d":"43.00"}]
[17,"Making  and  fixing  steel  grated  doors,  complete  with  locking arrangement, angle iron frame 2\"x2\"x3/8\" (50x50x10 mm) and\n¾\" (20 mm) square bars 4\" (100 mm) centre to centre.","SM",{"v":6,"d":"6.00"},{"v":24385.15,"d":"24,385.15"}]
[18,"Providing and fixing steel windows using M.S. sheet (16 SWG) moulded tubular pipe 1½\"x1½\" (40x40mm) for frame and 1¼\"x1¼\" (30x30mm) for leaves including M.S. square bars ¼\"x¼\" (6x6 mm) welded around each panel of frame, 5 mm thick glass panes fixed with double M.S. square tubular pipe 3/8\"x3/8\" (10x10mm) (22 SWG) beading with U' shaped rubber lining, brass fitting, holdfast, including painting three coats complete in all\nrespects."]
[null,"For  openable  panels  fixed  with  wire  gauze  24  SWG,  12x12\nmesh and glass panes ¼\" (6 mm) thick.","SM",{"v":3,"d":"3.00"},{"v":14435.35,"d":"14,435.35"}]
[19,"Distempering new Surface 3-Coats."]
[null,"one coat","SM",{"v":290,"d":"290.00"},{"v":95.1,"d":"95.10"}]
[null,"two coat","SM",{"v":290,"d":"290.00"},131.65]
[null,"three coat","SM",{"v":290,"d":"290.00"},{"v":168,"d":"168."}]
[20,"Dry brick on edge paving, sand grouted, including preparation of  bed  by  watering,  ramming  &  bringing  the  same  to  proper camber, by ½ \"(13 mm) thick mud plaster.","SM",{"v":49,"d":"49.00"},{"v":1618.1,"d":"1,618.10"}]
[21,"Painting  new  surface  Preparing  surface  and  painting  with\nemulsion paint:-"]
[null,"Prime coat","SM",{"v":34,"d":"34.00"}]
[null,"2nd and each subsequent coat","SM",{"v":34,"d":"34.00"}]
[22,"Fabrication  of  heavy  steel  work,  with  angle,  tees,  flat  iron round iron  and  sheet iron  for  making  trusses,  girders, tanks, etc.,  including cutting,  drilling, revitting, handling, assembling and   fixing,   but   excluding   erection   in   position.   For   Roof\nCanopy as per drawing.","kg",{"v":135,"d":"135.00"}]
[23,"Erection  and  fitting  in  position  iron  trusses,  staging  of  water\ntanks, etc.","kg",{"v":135,"d":"135.00"}]
[24,"Preparing of new surface\nc) Preparing surface and painting of doors and windows any type (including edges):-"]
[null,"Primer coat","SM",{"v":10,"d":"10.00"}]
[null,"Each subsequent coat","SM",{"v":10,"d":"10.00"}]
[25,"Filling, watering and ramming earth under floors:-\ni) with surplus earth from foundation, etc.","CM",{"v":61,"d":"61.00"}]
[26,"Providing and fixing, floor trap of cast iron, including concrete chamber all round, and C.I. grating:-\nii) 10x7.5 cm (4\"x3\")","Each",{"v":2,"d":"2.00"}]
[27,"Making and fixing deodar wood shelves, including brackets:-\ni) 1\" (25 mm) thick","SM",{"v":1,"d":"1.00"}]
[null,"MAKING GRID CONNECTION"]
[null,"Sub Head-VI"]
[null,"TUBE WELL (3 Cusecs)"]
[1,"Excavation of trenches in all kinds of soil, except cutting rock, for watersupply pipelines/electric cables upto 5 ft. (1.5 m) depth from ground level, including backfilling, trimming, dressing sides,leveling the beds of trenches to correct grade and cutting pits for joints, etc. complete in all respects.","CM",{"v":81,"d":"81.00"}]
[2,"Providing and fixing sluice valve of B.S.S. quality and weight, Class  `B',  for  cast  iron  pipe  line,  and  Asbestos  cement  pipe line (including cost of jointing material):-\ne) 8\" i/d (200 mm)","Each",{"v":2,"d":"2.00"}]
[3,"Providing  and  fixing  cast  iron  specials  of  B.S.S.  Class  'B' (such  as  bend,  tee,  cross  collar,  reducer,  tail  piece,  flanged socket, flanged spigot, cap, taper, angle branch, plug, etc) for Asbestos cement  pipe  line,  with comet  joint and rubber ring, complete.\nii) 8\" to 18\" (200 to 450 mm) i/d","P/kg",{"v":300,"d":"300.00"}]
[4,"Rehandling of earth work\na) Lead upto a single throw of Kassi, phaorah or shovel","CM",{"v":68,"d":"68.00"}]
[5,"Making connection for new watersupply lines with the running main,  including  excavation  of  trench  and  refilling,  complete, but  excluding  cost  of  pipe  and  specials,  etc.  Diameter  of running main:\nii) upto 8\" i/d (200 mm)","P.\nConnection",{"v":4,"d":"4.00"},{"v":5501.1,"d":"5,501.10"}]
[6,"Cement concrete plan l/c placing compacting finishing, curing complete (l/c screening and washing of store aggregate) 1:2:4","CM",{"v":1,"d":"1.00"},{"v":21779.18,"d":"21,779.18"}]
["TOTAL COST"]